Notes sur la calibration

“It is suggested that channel 5 is used because the higher the frequency the easier it is to observe step changes in the output.” p.104 user manual

“Operating at a wider bandwidth increases range but also increases power consumption. The DW1000 has fine control of the TX pulse width allowing optimum control of transmitted spectrum bandwidth.” P.211 user manual